#
DTC 05 ERR07 OR 05:ER07

BME090266900219

DTC 05 ERR07 or 05:Er07 | CD changer (external type)
DETECTION CONDITION |

  Note

  • When error occurs, error message "CHECK CD" is displayed in the LCD.

• Base unit detects CD reading error.
POSSIBLE CAUSE | • Defective CD (scratches or dirt) • CD changer (external type) malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY WHETHER MALFUNCTION IS IN CD CHANGER OR OTHER PARTS • Play all CD in magazine. • Is CD changer able to read them properly? | Yes | Go to Step 3.
No | Not able to change particular CD. | Go to next step.
Not able to change any CD. | Go to Step 3.
2 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
3 | INSPECT CD CHANGER (EXTERNAL TYPE) • Clear DTC. • Insert and play CD with no defect. • Start on-board diagnostic test mode. • Is DTC 05 ERR07 or 05:Er07 displayed? | Yes | Replace CD changer (external type).
No | Troubleshooting completed.