- AIR BAG SYSTEM
- NO.1 AIR BAG SYSTEM WARNING LIGHT DOES NOT ILLUMINATE WHEN IGNITION SWITCH IS TURNED TO ON POSITION
- NO.2 AIR BAG SYSTEM WARNING LIGHT ILLUMINATES IMMEDIATELY AFTER IGNITION SWITCH IS TURNED TO ON POSITION AND REMAINS ILLUMINATED
- NO.3 PASSENGER-SIDE AIR BAG CUT-OFF INDICATOR LIGHT DOES NOT DIM WHEN IGNITION SWITCH IS AT ON POSITION AND HEADLIGHT SWITCH IS TURNED TO TNS OR HEADLIGHT POSITION. (CHILD RESTRAINT SEAT BUILT IN RESONATOR IS ATTACHED TO PASSENGER-SIDE SEAT.)
- NO.4 PASSENGER-SIDE AIR BAG CUT-OFF INDICATOR LIGHT REMAINS DIMMED WHEN IGNITION SWITCH IS AT ON POSITION AND HEADLIGHT SWITCH IS TURNED OFF. (CHILD RESTRAINT SEAT BUILT IN RESONATOR IS ATTACHED TO PASSENGER-SIDE SEAT.)