#
ENGINE CONTROL SYSTEM DIAGRAM [MZR-CD (RF Turbo)]

BME014000140T03

.

1 | Air cleaner
2 | Vacuum chamber
3 | VBC check valve
4 | MAF/IAT sensor
5 | VBC solenoid valve
6 | Vacuum damper
7 | Guide blade actuator
8 | Turbocharger
9 | Charge air cooler
10 | IAT sensor No.2
11 | Boost sensor
12 | Intake shutter valve actuator
13 | Intake shutter solenoid valve (half)
14 | Intake shutter solenoid valve (full)
15 | EGR solenoid valve (vacuum)
16 | EGR solenoid valve (vent)
17 | EGR control solenoid valve
18 | EGR valve
19 | EGR water cooler
20 | VSC valve actuator
21 | VSC solenoid valve
22 | Fuel tank
23 | Fuel filter
24 | Fuel warmer
25 | Supply pump
26 | Suction control valve
27 | Fuel temperature sensor
28 | Common rail
29 | Fuel pressure sensor
30 | Fuel pressure limiter
31 | Glow plug
32 | Fuel injector
33 | ECT sensor
34 | Calibration resistor (With calibration resistor)
35 | CMP sensor
36 | Warm up oxidation catalytic converter
37 | Oxidation catalytic converter
38 | Silencer
39 | Vacuum pump
40 | CKP sensor
41 | Idle switch
42 | APP sensor
43 | Glow plug relay
44 | IDM
45 | PCM
46 | BARO sensor
47 | PCM control relay
48 | Engine switch
49 | Starter (starter signal)
50 | Neutral switch
51 | Clutch pedal position switch
52 | A/C switch
53 | CAN bus
54 | To PCM
55 | EGR valve position sensor
56 | DLC-2
57 | Fuel flow