#
ACCELERATOR PEDAL COMPONENT DISASSEMBLY/ASSEMBLY [MZR-CD (RF Turbo)]

BME011341600W03

1. Remove the accelerator pedal component. (See ACCELERATOR PEDAL COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Disassemble in the order indicated in the table.

1 | Idle switch
2 | Accelerator position sensor
3 | Accelerator pedal

3. Assemble in the reverse order of removal.

4. Install the accelerator pedal component. (See ACCELERATOR PEDAL COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

5. Adjust the accelerator position sensor. (See ACCELERATOR POSITION SENSOR ADJUSTMENT [MZR-CD (RF Turbo)].)

6. Adjust the idle switch. (See IDLE SWITCH ADJUSTMENT [MZR-CD (RF Turbo)].)