#
DTC 47

BME080201046W19

DTC 47 | Occupancy sensor (occupancy detection part)
DETECTION CONDITION |

  Warning

  • Detection conditions are for understanding DTC outline before performing inspection. Performing inspection with only detection conditions may cause injury due to operating error or damage the system. When performing inspection, always follow inspection procedure.

• Malfunction in occupancy sensor circuit

Diagnostic procedure

ACTION
Replace seat cushion. (See FRONT SEAT DISASSEMBLY/ASSEMBLY.)