#
SLIDING SUNROOF OUTLINE

BME091569800T01
• The function, structure and operation (side open/close and tilt up/down) is essentially carried over from the current 323 (BJ) model, except for the circuit in the sunroof motor and sunroof relay.
× : Applied

Item | MPV (LW)
--- | ---
Slide open/close function | ×
Auto-stop function (when closing) | ×
Tilt up/down function | ×
Number of limit switch | 3
Sliding amount | (mm {in}) | 633 {24.9}
Tilt up | (mm {in}) | 28 {1.1}