#
VENTILATOR GRILLE REMOVAL/INSTALLATION

BME091764730201

## Driver's Side and Center

1. Remove the meter hood.

2. Remove the screws from behind the center panel, and remove the ventilator grille.

3. Install in the reverse order of removal.

## Passenger's Side

1. Remove the dashboard. (See DASHBOARD REMOVAL/INSTALLATION.)

2. Remove the screws from behind the dashboard, then remove the ventilator grille.

3. Install in the reverse order of removal.