#
OIL PAN CONSTRUCTION [L3]

BME011110040T03

## Construction

• An aluminum alloy oil pan has been adopted for weight reduction. A silicone sealant with excellent sealing qualities has been adopted on the oil pan gasket.
• An oil pan baffle plate made of steel has been adopted on the interior of the oil pan to improve engine oil diffusion from the crankshaft rotation, and to maintain the oil level during vehicle roll.

1 | Oil pan baffle plate