#
DIFFERENTIAL DISASSEMBLY

BME051527100M02

1. Disassemble in the order indicated in the table.

A65M-R

.

1 | Ring gear
2 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Disassembly Note.)
3 | Spacer
4 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Disassembly Note.)
5 | Gear case component

A65MX-R

.

1 | Ring gear
2 | Bearing (ring gear-opposite side) (See Bearing (Ring Gear-Opposite Side) Disassembly Note.)
3 | Spacer
4 | Speedometer drive gear
5 | Reduction gear
6 | Bearing (ring gear side) (See Bearing (Ring Gear Side) Disassembly Note.)
7 | Gear case component

## Bearing (Ring Gear-Opposite Side) Disassembly Note

1. Remove the bearing using the SST.

## Bearing (Ring Gear Side) Disassembly Note

1. Remove the bearing using the SSTs.

A65M-R

A65MX-R