#
THIRD-ROW SEAT DISASSEMBLY/ASSEMBLY

BME09135730XW03

## TYPE A

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Headrest
2 | Pole guide
3 | Knuckle upper cover
4 | Seat back rear cover
5 | Seat back trim
6 | Seat back pad
7 | Seat back frame
8 | Seat under bracket side cover
9 | Seat under bracket
10 | Seat under bracket upper cover
11 | Seat cushion trim
12 | Seat cushion pad
13 | Seat cushion frame
14 | Recliner lever
15 | Side cover
16 | Reverse cover
17 | Recliner knuckle
18 | Third-row buckle
19 | Slide adjuster

## TYPE B

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Headrest
2 | Pole guide
3 | Seat back trim
4 | Seat back pad
5 | Seat back frame
6 | Seat cushion under cover
7 | Cover
8 | Seat cushion trim
9 | Seat cushion pad
10 | Hinge cover
11 | Recliner knuckle cover
12 | Recliner knuckle
13 | Cable
14 | Catch