#
SYSTEM WIRING DIAGRAM

BME091258000T04

.

1 | Power window main switch
2 | Close relay
3 | Open relay
4 | Pulse generator
5 | Limit switch
6 | Front power window regulator (Driver's side)
7 | Front power window regulator (Passenger's side)
8 | Rear power window regulator (Right side)
9 | Rear power window regulator (Left side)
10 | Power window subswitch
11 | Manual close
12 | Manual open
13 | Auto
14 | Power-cut switch
15 | Close
16 | Open
17 | Door switch (Driver's side)
18 | Door switch (Passenger's side)
19 | Door switch (Rear right side)
20 | Door switch (Rear left side)