#
CONTROL SYSTEM WIRING DIAGRAM [L3]

BME014000000T84

## With Immobilizer System

1 | HO2S (front)
2 | HO2S (rear)
3 | TP sensor
4 | MAP sensor
5 | BARO sensor
6 | ECT sensor
7 | MAF/IAT sensor
8 | IAT sensor
9 | MAF sensor
10 | DLC-2
11 | Knock sensor
12 | CKP sensor
13 | CMP sensor
14 | Fuel injector No.1
15 | Fuel injector No.2
16 | Fuel injector No.3
17 | Fuel injector No.4
18 | IAC valve
19 | HO2S heater (front)
20 | HO2S heater (rear)
21 | A/C relay
22 | Fan control module
23 | Fuel pump relay
24 | Immobilizer unit
25 | Instrument cluster
26 | Ignition switch
27 | Main relay
28 | PCM
29 | Generator
30 | Refrigerant pressure switch (middle)
31 | PSP switch
32 | Blower motor
33 | Refrigerant pressure switch (high and low)
34 | A/C switch
35 | Brake switch
36 | Stop light
37 | Neutral switch
38 | Clutch switch
39 | DLC
40 | Instrument cluster
41 | Ignition coil
42 | Purge solenoid valve
43 | EGR valve
44 | Variable tumble control solenoid valve
45 | VIS control solenoid valve
46 | Instrument cluster
47 | PCM
48 | European (L.H.D. U.K.) specs.
49 | Except for European (L.H.D. U.K.) specs.
50 | Generator warning light
51 | TCS HU/CU
52 | Battery
53 | VSS
54 | PCM terminal 4V
55 | Input turbine speed sensor
56 | TR switch
57 | HOLD indicator light
58 | HOLD switch
59 | Oil pressure switch
60 | TFT sensor
61 | Ignition switch (STA)
62 | Down shift solenoid
63 | Pressure control solenoid

## Without Immobilizer system

1 | HO2S (front)
2 | HO2S (rear)
3 | TP sensor
4 | MAP sensor
5 | BARO sensor
6 | ECT sensor
7 | MAF/IAT sensor
8 | IAT sensor
9 | MAF sensor
10 | DLC-2
11 | Knock sensor
12 | CKP sensor
13 | CMP sensor
14 | Fuel injector No.1
15 | Fuel injector No.2
16 | Fuel injector No.3
17 | Fuel injector No.4
18 | IAC valve
19 | HO2S heater (front)
20 | HO2S heater (rear)
21 | A/C relay
22 | Fan control module
23 | Fuel pump relay
24 | Pressure control solenoid
25 | Instrument cluster
26 | Ignition switch
27 | Main relay
28 | PCM
29 | Generator
30 | Refrigerant pressure switch (middle)
31 | PSP switch
32 | Blower motor
33 | Refrigerant pressure switch (high and low)
34 | A/C switch
35 | Brake switch
36 | Stop light
37 | Neutral switch
38 | Clutch switch
39 | DLC
40 | Instrument cluster
41 | Ignition coil
42 | Purge solenoid valve
43 | EGR valve
44 | Variable tumble control solenoid valve
45 | VIS control solenoid valve
46 | Instrument cluster
47 | PCM
48 | European (L.H.D. U.K.) specs.
49 | Except for European (L.H.D. U.K.) specs.
50 | Generator warning light
51 | TCS HU/CU
52 | Battery
53 | VSS
54 | PCM terminal 4V
55 | Input turbine speed sensor
56 | TR switch
57 | HOLD indicator light
58 | HOLD switch
59 | Oil pressure switch
60 | TFT sensor
61 | Ignition switch (STA)
62 | Down shift solenoid