#
CONTROL SYSTEM WIRING DIAGRAM

BME074000000T02

Front

.

1 | Front climate control unit
2 | Air intake actuator
3 | Front blower motor
4 | Front resistor
5 | Thermosensor
6 | Refrigerant pressure switch
7 | Magnetic clutch
8 | A/C relay
9 | Front blower relay
10 | Front fan switch
11 | Rear window defroster switch
12 | Rec/fresh switch
13 | A/C switch
14 | Microswitch
15 | A/C 10 A fuse
16 | HEATER 40 A fuse
17 | ROOM 10 A fuse
18 | Amplifier
19 | RECIRCULATE
20 | FRESH
21 | To instrument cluster

Rear

.

1 | Rear climate control unit
2 | Air mix actuator
3 | Airflow mode actuator
4 | Rear blower motor
5 | Rear resistor
6 | Rear blower relay
7 | Rear main fan switch
8 | Rear fan switch
9 | A/C 10 A fuse
10 | R.HEATER 30 A fuse
11 | VENT
12 | BI-LEVEL
13 | HEAT
14 | COLD
15 | HOT
16 | Rear cooler and rear heater only