#
VEHICLE SPEEDOMETER SENSOR DESCRIPTION [JA5A-EL]

BME051719200T10

## Function

• A vehicle speedometer sensor is located in the transaxle case and detects the rotating speed of the parking gear.

## Construction/Operation

• The magnetic pickup type of vehicle speedometer sensor is mounted in the transaxle case, next to the parking gear. It generates a 18-pulse signal for each rotation of the parking gear, and sends this signal to the TCM.