#
DTC 07 ERR02 OR 07:ER02

BME090266900W24

DTC 07 ERR02 or 07:Er02 | MD player
DETECTION CONDITION |

  Note

  • When error occurs, error message "CHECK MD" is displayed in the LCD.

• Cannot play MD normally or change tracks.
POSSIBLE CAUSE | • Defective MD (scratches or dirt) • MD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY WHETHER MALFUNCTION IS IN MD PLAYER OR MD • Play MD and select other song (change tracks). • Is MD player able to change tracks? | Yes | Go to Step 3.
No | Not able to change particular tracks. | Go to next step.
Not able to change any tracks. | Change MD and perform track-change again. • If MD player changes tracks, then go to Step 3. • If not, replace MD player.
2 | INSPECT MD • Inspect condition of MD where error has occurred. • Is MD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace MD, then go to next step.
3 | INSPECT MD PLAYER • Clear DTC. • Play MD and select other song (change tracks). • Start on-board diagnostic test mode. • Is DTC 07 ERR02 or 07:Er02 displayed? | Yes | Replace MD player.
No | Troubleshooting completed.