#
REAR BRAKE (DISC) REMOVAL/INSTALLATION

BME041126980202

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, do the following.

  (1) Depress the brake pedal a few times. Then verify that the brakes do not drag.
  (2) Inspect the pedal-to-floor clearance.
  (3) Inspect the parking brake lever stroke.

1 | Brake hose
2 | Caliper
3 | Disc pad (See Disc Pad Installation Note)
4 | Outer shim
5 | Inner shim
6 | Guide plate
7 | Mounting support
8 | Dust boot
9 | Disc plate

## Disc Pad Installation Note

1. Push the piston fully inward using the SST.

2. Install the disc pad.