#
DRIVELINE/AXLE TECHNICAL DATA

BME035000000W01

Item | Specification
--- | ---
Engine type | L3 | MZR-CD (RF Turbo)
Front axle | Maximum wheel bearing play | (mm {in}) | 0.05 {0.002}
Rear axle | Maximum wheel bearing play | (mm {in}) | 0.05 {0.002}
Front drive shaft | Shaft length (Air in boot at atmospheric pressure) | (mm {in}) | Left side | 644.7-654.7 {25.39-25.77} | 640.7-650.7 {25.23-25.61}
Right side | 594.7-604.7 {23.42-23.80} | 564.7-574.7 {22.24-22.62}