#
FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION

BME041343720W03

1. Remove the air cleaner (L3 ). (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].)

2. For the MZR-CD (RF Turbo) engine model, remove the fuel filter installation bolt and put the fuel filter aside. (See FUEL FILTER COMPONENT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

.

1 | Connector
2 | Bolt
3 | Front ABS wheel-speed sensor