#
ENGINE FEATURES

BME010002000102

## On-board diagnostic system

To meet the EOBD regulations | • Diagnostic test modes adopted (MZR-CD (RF Turbo))
Improved serviceability | • DTC troubleshooting modified (MZR-CD (RF Turbo)) • PID/DATA monitor items added (MZR-CD (RF Turbo)) • Simulation items added (MZR-CD (RF Turbo)) • OBD drive mode adopted (MZR-CD (RF Turbo))

## Lubrication system

Improved lubricity and reliability | • Engine oil capacity has been changed (AJ) • Engine oil type has been changed

## Control System

Improved emission performance | • A EGR valve position sensor has been adopted (MZR-CD (RF Turbo))
Wiring harness simplification | • CAN adopted (MZR-CD (RF Turbo))