#
POWER SLIDING DOOR (PSD) SYSTEM WIRING DIAGRAM

BME091101085T05

LH PSD system (RH same as LH)

1 | Latch position switch (LH)
2 | Easy closure motor (LH)
3 | Easy closure control module (LH)
4 | Sliding door lock-link switch (LH)
5 | Unlock
6 | ABS warning light
7 | Release
8 | Latch release actuator (LH)
9 | Sliding door circuit contact (LH)
10 | PSD drive module (LH)
11 | PSD motor
12 | Close
13 | Open
14 | Brake solenoid
15 | Speed sensor
16 | Check switch
17 | Child safety lock switch
18 | PSD control module (LH)
19 | To RH PSD system
20 | Instrument cluster
21 | Vehicle speed signal output
22 | Door ajar warning light
23 | Brake system warning light
24 | Brake switch
25 | Door switch (LR)
26 | Door switch (LF)
27 | Parking brake switch
28 | P position switch
29 | Cargo compartment light switch
30 | Brake light
31 | Keyless unit
32 | PSD rear switch (LH)
33 | PSD front switch
34 | PSD rear switch (RH)
35 | Open/close switch (LH)
36 | Main switch
37 | Open/close switch (RH)
38 | ABS HU/CM