#
NO.22 VIBRATION CONCERNS (ENGINE) [L3]

BME010300000W24

22 | VIBRATION CONCERNS (ENGINE)
--- | ---
DESCRIPTION | • Vibration from under hood or driveline
POSSIBLE CAUSE | • Loose attaching bolts or worn parts • Components malfunction such as worn parts

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Inspect following components for loose attaching bolts or worn parts: • Cooling fan • Condenser fan • Drive belt and pulleys • Engine mounts
All items okay?
Yes
Inspect following systems:
• Wheels
• Driveline
• Suspension
No | Readjust or retighten engine mount installation position. Service if necessary for other parts.
2 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM.