#
SECOND-ROW SEAT DISASSEMBLY/ASSEMBLY

BME09135720X203

## TYPE A

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Headrest
2 | Pole guide
3 | Knuckle upper cover
4 | Seat back rear cover
5 | Seat back trim
6 | Seat back pad
7 | Seat back frame
8 | Seat under bracket side cover
9 | Seat under bracket
10 | Seat under bracket upper cover
11 | Seat cushion trim
12 | Seat cushion pad
13 | Seat cushion frame
14 | Recliner lever
15 | Side cover
16 | Reverse cover
17 | Recliner knuckle
18 | Second-row buckle
19 | Second-row seat belt (center only)
20 | Slide adjuster

## TYPE B

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Headrest
2 | Pole guide
3 | Side cover No.1
4 | Armrest trim
5 | Armrest pad
6 | Knuckle upper cover
7 | Seat back rear cover
8 | Seat back trim
9 | Seat back pad
10 | Seat back frame
11 | Seat under bracket side cover
12 | Seat under bracket (Right)
13 | Seat under bracket (Left)
14 | Seat cushion trim
15 | Seat cushion pad
16 | Seat cushion frame
17 | Recliner lever
18 | Side cover No.2
19 | Reverse cover
20 | Recliner knuckle
21 | Second-row buckle
22 | Slide adjuster

## TYPE C

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Cup holder (Right side seat only)
2 | Headrest
3 | Pole guide
4 | Side cover No.1
5 | Armrest trim
6 | Armrest pad
7 | Knuckle upper cover
8 | Seat back rear cover
9 | Seat back trim
10 | Seat back pad
11 | Seat back frame
12 | Seat under bracket side cover
13 | Seat under bracket
14 | Seat under bracket upper cover
15 | Seat cushion trim
16 | Seat cushion pad
17 | Seat cushion frame
18 | Recliner lever
19 | Side cover No.2
20 | Reverse cover
21 | Recliner knuckle
22 | Second-row buckle
23 | Slide adjuster