#
IGNITION COIL CONSTRUCTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed))

BME011818100T03
• The coil on the plug ignition operates similar to standard coil pack ignition except each plug has one coil per plug. The electric wiring system of the coil on the plug ignition is indicated in the figure below.

1 | To PCM
2 | IG1
3 | PCM
4 | Cylinder number
5 | Ignition coil