#
FRONT STABILIZER REMOVAL/INSTALLATION

BME021334100201

1. Remove the crossmember. (See FRONT CROSSMEMBER REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

1 | Stabilizer control link
2 | Stabilizer bracket (See Stabilizer Bracket Installation Note.)
3 | Stabilizer bushing
4 | Front stabilizer

3. Install in the reverse order of removal.

4. Inspect the front wheel alignment and adjust it if necessary.

## Stabilizer Bracket Installation Note

1. Apply rubber grease to the inside surface of the stabilizer bushing.

2. Align the bushing with the inside of the positioning plate on the stabilizer bar.

3. Install the stabilizer bracket.