#
DRIVE INFORMATION SYSTEM SWITCH REMOVAL/INSTALLATION

BME092201067W01

1. Disconnect the negative battery cable.

2. Remove the driver-side side panel.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Drive information system switch (See Drive Information System Switch Removal Note.)
2 | Connector

## Drive Information System Switch Removal Note

1. Insert your hand into the hole for the driver-side side panel, grasp the tabs of the drive information system switch and pull it forward to remove it.