#
DTC 03 ERR01 OR 03:ER01

BME090266900W12

DTC 03 ERR01 or 03:Er01 | CD player
DETECTION CONDITION | • CD player cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective CD (broken or foreign material stuck/attached) • CD player malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is CD able to be ejected? | Yes | Go to next step.
No | Replace CD player.
2 | INSPECT CD • Inspect condition of CD where error has occurred. • Is CD okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace CD, then go to next step.
3 | INSPECT CD PLAYER • Clear DTC. • Insert and eject CD with no defect. • Start on-board diagnostic test mode. • Is DTC 03 ERR01 or 03:Er01 displayed? | Yes | Replace CD player.
No | Troubleshooting completed.