#
IMMOBILIZER SYSTEM OUTLINE

BME091467000T01
• The immobilizer system is the same as that of the current MPV (LW) model.

Comparison with previous MPV (LW) model

× : Applied

Item | Comparison
--- | ---
European (L.H.D. U.K.) specs. (except AJ) | Australian, European (L.H.D.) (AJ), General (L.H.D. R.H.D.) specs.
System operation | Same as the current XEDOS 9 (TA) model | Same as the previous MPV (LW) model
Key reminder switch ON/OFF detection function | × | -
Starter relay control function | × | -
On-board diagnostic function | × | ×