#
ON-BOARD DIAGNOSTIC OUTLINE [MZR-CD (RF Turbo)]

BME010200102T08
• The on-board diagnostic system for Mazda MPV has been adopted or changed the following parts.

  - DTCs, PID monitoring items, and simulation items have been added.
  - A MIL has been adopted to indicate malfunctions in the engine control system.
  - A DLC-2 has been added to communicate with the WDS or equivalent.
  - A KOEO/KOER self-test function has been adopted. Accordingly, the present malfunction or a successful repair is readily confirmed.