#
FUEL PUMP UNIT DISASSEMBLY/ASSEMBLY [L3]

BME011413350W02

  Warning

  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injuries or death and damage. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel pump unit when removing or installing.

1. Disassemble in the order indicated in the table.

1 | Fuel pump unit cover
2 | Fuel filter (high-pressure)
3 | Spacer
4 | Rubber mount
5 | Fuel filter (low-pressure)
6 | Fuel pump
7 | Fuel gauge sender unit

2. Assemble in the reverse order of disassembly.