#
CYLINDER BLOCK (I) DISASSEMBLY

A6E242402000E07

1. Disassemble in the order indicated in the table.

1 | Oil pan
2 | Oil filter cover
3 | Oil filter
4 | Oil filter adapter
5 | Oil cooler
6 | Knock sensor
7 | Oil separator
8 | Thermostat
9 | Water pump
10 | Oil strainer
11 | Oil pump
12 | Flywheel (MTX ), Drive plate (ATX) (See Drive Plate (ATX), Flywheel (MTX) Disassembly Note)
13 | End plate (MTX)
14 | Rear oil seal

## Drive Plate (ATX), Flywheel (MTX) Disassembly Note

1. Hold the crankshaft using the SST.

2. Remove the bolts in several passes.