#
IGNITION COIL CONSTRUCTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)

BME011818100T02
• The coil on the plug ignition operates similar to standard coil pack ignition except each plug has one coil per plug. The electric wiring system of the coil on the plug ignition is indicated in the figure below.

1 | To PCM
2 | IG1
3 | PCM
4 | Cylinder number
5 | Ignition coil