#
SECONDARY SHAFT COMPONENTS DISASSEMBLY

BME051517301302

1. Disassemble in the order indicated in the table.

1 | Bearing (See Bearing and Secondary 4th Gear Disassembly Note)
2 | Secondary 4th gear
3 | Retaining ring
4 | Secondary 3rd gear (See Secondary 3rd Gear and 2nd Gear Disassembly Note)
5 | 2nd gear
6 | 2nd synchronizer ring
7 | Retaining ring
8 | 1st/2nd clutch hub component (See 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note)
9 | 1st synchronizer ring
10 | 1st gear
11 | Bearing (secondary shaft end) (See Bearing (Secondary Shaft End) Disassembly Note)
12 | Secondary shaft gear
13 | Synchronizer key springs
14 | Clutch hub sleeve (reverse gear)
15 | Synchronizer keys
16 | 1st/2nd clutch hub

## Bearing and Secondary 4th Gear Disassembly Note

1. Remove the bearing and secondary 4th gear using the SST.

## Secondary 3rd Gear and 2nd Gear Disassembly Note

1. Remove the retaining ring.

2. Shift the gears to 1st gear.

3. Remove the secondary 3rd gear and 2nd gear using the SST.

## 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note

1. Remove the retaining ring.

2. Remove the 1st/2nd clutch hub component, 1st synchronizer ring, and 1st gear using a press.

## Bearing (Secondary Shaft End) Disassembly Note

1. Remove the bearing using the SST.