#
BODY SHELL CABIN CONSTRUCTION

BME091056100T04
• To protect passengers in collisions from various directions, the passenger cabin constructed follows:

  - The B-pillar inner and B-pillar reinforcement are thicker.
  - The pillar configuration is designed to prevent pillar intrusions into the cabin during a collision. A thicker pillar had increased its strength.

1 | Collision energy
2 | Side sill reinforcement
3 | Torque box No.2
4 | Torque box No.3
5 | Crossmember No.3
6 | Crossmember No.4
7 | B-pillar reinforcement
8 | B-pillar inner
9 | Front pillar reinforcement
10 | Roof reinforcement
11 | Sec. A-A