#
CONVENTIONAL BRAKE SYSTEM LOCATION INDEX

BME041100000W01

.

1 | Vacuum hose check valve (See VACUUM HOSE CHECK VALVE INSPECTION (POWER BRAKE UNIT))
2 | Brake pedal (See BRAKE PEDAL INSPECTION) (See BRAKE PEDAL REMOVAL/INSTALLATION)
3 | Brake switch (See BRAKE SWITCH INSPECTION)
4 | Master cylinder (See MASTER CYLINDER REMOVAL/INSTALLATION) (See MASTER CYLINDER DISASSEMBLY/ASSEMBLY)
5 | Fluid level sensor (See FLUID LEVEL SENSOR INSPECTION)
6 | Power brake unit (See POWER BRAKE UNIT INSPECTION) (See POWER BRAKE UNIT REMOVAL/INSTALLATION)
7 | Brake pipe joint (See BRAKE PIPE JOINT REPLACEMENT)
8 | Front brake (disc) (See FRONT BRAKE (DISC) INSPECTION) (See FRONT BRAKE (DISC) REMOVAL/INSTALLATION)
9 | Disc pad (front) (See DISC PAD (FRONT) REPLACEMENT)
10 | Caliper (front) (See CALIPER (FRONT) DISASSEMBLY/ASSEMBLY)
11 | Rear brake (drum) (See REAR BRAKE (DRUM) INSPECTION) (See REAR BRAKE (DRUM) REMOVAL/INSTALLATION)
12 | Wheel cylinder (See WHEEL CYLINDER DISASSEMBLY/ASSEMBLY)