#
AUDIO UNIT REMOVAL/INSTALLATION

BME092066900202

1. Disconnect the negative battery cable.

2. Remove the meter hood.

3. Remove in the order indicated in the table.

  Caution

  • Make certain that the wiring harness and antenna feeder are not caught between the unit and dashboard. If the harness or the antenna feeder is caught between the unit and dashboard, it may cause trouble or malfunctions.

4. Install in the reverse order of removal.

1 | Screw
2 | Connector
3 | Audio unit