#
INTAKE-AIR SYSTEM OUTLINE [AJ]

BME011300000T06
• The intake-air system for Mazda MPV has been adopted or changed the following parts.

  - The Intake Manifold Communication Control (IMCC) system components have been adopted, that same function as the Variable resonance induction system (VRIS).
  - The IAC valve has been changed.

Item | Remark for new model
--- | ---
Fresh-air duct | Same function as previous MPV (LW) GY engine models
Resonance chamber | Same function as previous MPV (LW) GY engine models
Air cleaner | Same function as previous MPV (LW) GY engine models
IAC valve | Same as current TRIBUTE (U0) AJ engine models
Throttle body | Same function as previous MPV (LW) GY engine models
Dynamic chamber | Same function as previous MPV (LW) GY engine models
Intake manifold | Same function as previous MPV (LW) GY engine models
IMCC system | Same function as current Xedos9 and Eunos 800 (TA) KL engine models