24341AX107
2	0.3	26AR	KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH	M004
3	0.5	LP	PROTECTED + SIDE LIGHT FEED	M004
6	0.5	20G	TAILGATE MOTOR OPEN CONTROL 	M004
7	0.5	H66P	REVERSING LIGHTS + CONTROL	M004
