| CONNECTION
ANY TYPE

#### R374
REAR LEFT-HAND WIRING / FRONT WIRING HARNESS CONNECTION
H45/DG TR4X4/RAD02,RAD04,RAD05

4 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | M049
5 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | M049
13 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | M049
14 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | M049
15 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | M049
16 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | M049