| CONNECTION
ANY TYPE

#### R324
SEAT / LEFT-HAND SEAT ELECTRICAL FUNCTIONS
H45/DG TR4X4/RAD02,RAD04,RAD05

1 | 0.3 | LP | PROTECTED + SIDE LIGHT FEED | ?????
2 | 0.3 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | 79A | HEATED SEAT + CONTROL | ?????
5 | 1.2 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
6 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
7 | 0.5 | 60EE | FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL | ?????
8 | 1.2 | BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW | ?????