| CONNECTION
ANY TYPE

#### R4
DASHBOARD/PASSENGER'S DOOR CONNECTION
H45/DG FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD02/BVM6

3 | 0.3 | 26CG | PASSENGER DOOR SWITCH/LOCKING SIGNAL | F049
4 | 0.3 | 26AD | KEYLESS VEHICLE FRONT RIGHT DOOR EXTERNAL AERIAL SIGNAL 2 | F049
5 | 0.3 | 26AC | KEYLESS VEHICLE FRONT PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | F049
8 | 0.5 | 15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL | F049
9 | 0.5 | 40E | REAR VIEW MIRROR MOTOR COMMON | F049
10 | 0.5 | 40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL | F049
14 | 0.3 | 26Q | PASSENGER SIDE DOOR HANDLE INFRARED SENSOR SIGNAL | F049
15 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | F049
16 | 0.5 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL | F049
17 | 0.5 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL | F049
19 | 0.3 | 23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL | F049
20 | 0.5 | 13C | INTERIOR LIGHT - CONTROL | F049
21 | 0.5 | BPT | PROTECTED + BATTERY FEED TIMER | F049
22 | 0.5 | 40W | REAR-VIEW MIRROR FOLD IN CONTROL | F049
23 | 0.5 | 40X | REAR-VIEW MIRROR FOLD OUT CONTROL | F049
24 | 0.5 | 40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL | F049