| DASHBOARD WIRING
H45/DD

#### 261
RADIO
FMMANU,FPAUTO/RDAVAR/SOP01/RETRCR/LVILVE/NINAV1/BVM6

A1 | 0.5 | 47F | VEHICLE SPEED SIGNAL | CT2F
B1 | 0.5 | 34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL | CT2F
B2 | 0.5 | 34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL | CT2F
B3 | 0.5 | 34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL | CT2F
A4 | 0.85 | BP26 | CARPHONE PROTECTED + BATTERY FEED | CT2F
B4 | 0.5 | 34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL | CT2F
B5 | 0.5 | 34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL | CT2F
B6 | 0.5 | 34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL | CT2F
B7 | 0.5 | 34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL | CT2F
A8 | 2.0 | MT | RADIO ELECTRICAL EARTH | ?????
B8 | 0.5 | 34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL | CT2F