| LEFT-HAND REAR DOOR WIRING
H45

#### 131
REAR LEFT-HAND ELECTRIC WINDOW CONTROL
DG,DD/LVILVE/NINAV2/RAD03

2 | 0.5 | MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
4 | 1.2 | 23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1 | ?????
5 | 1.2 | 23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE | ?????
6 | 1.2 | 23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN | ?????
7 | 1.2 | 23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2 | ?????
8 | 1.2 | A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY | ?????