| DASHBOARD WIRING
H45/DG

#### 645
PASSENGER COMPARTMENT COMPUTER
FPAUTO/RDAVAR/SOP03/RETRCR/LVILVI/RAD05/BVM6

37 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
38 | 0.3 | 87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
3 | 0.3 | 26AW | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2 | ?????
4 | 0.3 | 26AV | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1 | ?????
7 | 0.3 | 26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2 | ?????
8 | 0.3 | 26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL | ?????
16 | 0.3 | A5 | ENGINE AFTER IGNITION CONTROL RELAY | ?????
21 | 0.5 | 5HT | STARTER RELAY CONTROL | ?????
30 | 0.3 | 26AR | KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH | ?????
33 | 0.3 | 26P | DOOR HANDLE INFRARED SENSOR + | ?????
34 | 0.5 | 36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL | ?????
35 | 0.5 | 87T | BOOT LID POSITION SWITCH 1 SIGNAL | ?????
36 | 0.5 | 20G | TAILGATE MOTOR OPEN CONTROL | ?????