24341AX119
1	0.5	87T	BOOT LID POSITION SWITCH 1 SIGNAL	M004
2	0.3	26AR	KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH	M004
3	0.3	26AV	KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1	M004
5	0.5	87A	LEFT HAND REAR 1st POSITION SWITCH - SIGNAL	M004
6	0.5	87H	DRIVER'S 1st POSITION SWITCH - SIGNAL	M004
7	0.5	34MB	RADIO SOCKET AUXILIARY INPUT SIGNAL	M004
8	0.3	LP	PROTECTED + SIDE LIGHT FEED	M004
9	0.5	151R	BUZZER +	M004
10	0.5	35N	FRONT LOUDSPEAKER SIGNAL	M004
11	0.3	70BS	LEFT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY	M004
12	0.3	70BT	LEFT-HAND REAR WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL	M004
13	0.3	47F	VEHICLE SPEED SIGNAL	M004
14	0.5	BPT	PROTECTED + BATTERY FEED TIMER	M004
15	0.5	AP44	POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION	M004
17	0.85	20S	TAILGATE MOTOR OPENING AUTHORISED FEED	?????
18	0.5	20G	TAILGATE MOTOR OPEN CONTROL 	M004
19	0.3	26AW	KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2	M004
22	0.3	MZS	LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT	M004
23	0.5	TB45	RADIO SOCKET AUXILIARY SOCKET INPUT SHIELDED CABLE	M004
24	0.5	34MA	RADIO SOCKET AUXILIARY INPUT SIGNAL	M004
25	0.5	151E	PARKING AID WARNING LIGHT CONTROL	M004
26	0.5	151W	PARKING AID DEACTIVATION	M004
27	0.3	70BV	LEFT-HAND REAR WHEEL AERIAL RECEIVER EARTH	M004
28	0.3	70BU	LEFT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL	M004
29	0.5	60EE	FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL	M004
30	0.5	13E	INTERIOR LIGHTS - CONTROL > TIMER	M004
31	0.5	64C	LEFT HAND TURN SIGNAL LIGHTS CONTROL	M004
