| CONNECTION
ANY TYPE

#### R450
DASHBOARD/RIGHT REAR 3
H45/DG FMMANU/SOP01/LVILVE/RAD02/BVA6/BVVR

1 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | ?????
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
2 | 0.5 | 60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH | ?????
9 | 0.3 | 87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL | ?????
10 | 0.5 | 60DS | PASSENGER AIR BAG INHIBITOR KEY SIGNAL | ?????
11 | 0.5 | LP | PROTECTED + SIDE LIGHT FEED | ?????
20 | 0.3 | 87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL | ?????