103A | HEADLIGHT POSITION CONTROL
107E | RADIO SOUND CUT-OFF SIGNAL FOR TELEPHONE
107F | MULTIMEDIA MICROPHONE SIGNAL
107G | HANDS FREE TELEPHONE MICROPHONE +
107J | TELEPHONE MICROPHONE SCREENING
107L | TELEPHONE AUDIO + SIGNAL
107M | TELEPHONE AUDIO - SIGNAL
107W | DIAGNOSTIC SOCKET CANH MULTIMEDIA SIGNAL
107X | DIAGNOSTIC SOCKET CANL MULTIMEDIA SIGNAL
115A | OIL TEMPERATURE SENSOR - SIGNAL
11S | RIGHT-HAND PROTECTED SIDE LIGHT +CONTROL
11T | LEFT-HAND PROTECTED SIDE LIGHT +CONTROL
13C | INTERIOR LIGHT - CONTROL
13CA | PASSENGER STORAGE COMPARTMENT LIGHT CONTROL
13E | INTERIOR LIGHTS - CONTROL > TIMER
141B | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 1 SIGNAL
141C | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 2 SIGNAL
141D | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 3 SIGNAL
141G | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 4 SIGNAL
141H | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL LINE 5 SIGNAL
141K | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 1 SIGNAL
141L | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 2 SIGNAL
141M | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 3 SIGNAL
141N | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 4 SIGNAL
141P | INFORMATION DISPLAY STEERING WHEEL MOUNTED CONTROL COLUMN 5 SIGNAL
14K | WINDSCREEN WIPER TIMER LOW SPEED + CONTROL
14L | WINDSCREEN WIPER TIMER HIGH SPEED + CONTROL
14M | WINDSCREEN WIPER PARK POSITION CONTROL > COMPUTER
14S | RAIN SENSOR SERIAL LINE SIGNAL
150D | STATIC LOCKING CONTROL
150G | STATIC UNLOCKING CONTROL
150H | LOCKING INDICATOR LIGHT CONTROL
150K | CLUTCH SENSOR SIGNAL
150L | CLUTCH - SENSOR
150N | DYNAMIC BRAKE ACTUATOR SIGNAL
150P | DYNAMIC BRAKE - ACTUATOR
150Q | CLUTCH SENSOR +
151C | EXTERIOR LEFT HAND REAR SENSOR SIGNAL
151E | PARKING AID WARNING LIGHT CONTROL
151H | EXTERIOR RIGHT HAND REAR SENSOR SIGNAL
151M | INTERIOR LEFT HAND REAR SENSOR SIGNAL
151Q | INTERIOR RIGHT HAND REAR SENSOR SIGNAL
151R | BUZZER +
151S | BUZZER CONTROL
151U | EXTERIOR + SENSOR
151V | EXTERIOR - SENSOR
151W | PARKING AID DEACTIVATION
15B | HEATED REAR SCREEN + CONTROL
15LP | PROTECTED HEATED REAR SCREEN + CONTROL
15M | HEATED REAR SCREEN RELAY - CONTROL
15RP | PROTECTED HEATED REAR VIEW MIRROR + CONTROL
16A | WINDSCREEN WASHER PUMP + CONTROL
174A | COMMUNICATION SIGNAL BETWEEN UCH AND IMMOBILISER COMPUTER
176C | TELEVISION + IMAGE OUTPUT + SIGNAL
176D | TELEVISION IMAGE EARTH
179A | MOBILE PHONE HEADPHONE SOCKET TRANSMISSION SIGNAL
179B | MOBILE PHONE HEADPHONE SOCKET RECEPTION SIGNAL
179C | MOBILE PHONE HEADPHONE SOCKET EARTH
179D | MOBILE PHONE HEADPHONE SOCKET SECRET MODE CONTROL
17A | GLOVE COMPARTMENT LIGHTS - CONTROL
19F | + DIMMER FEED
1A | STARTER SOLENOID + CONTROL > RELAY
20AR | DEADLOCKING MOTOR CONTROL
20AW | ONE-TOUCH DOOR LOCKING/UNLOCKING CONTROL
20BC | DRIVER'S DOOR / FUEL FILLER FLAP UNLOCKING MOTOR CONTROL
20BD | OPEN FRONT/REAR PASSENGER DOORS MOTOR CONTROL
20D | ELECTRIC DOOR LOCKS CLOSE + CONTROL
20DC | DRIVER'S DOOR LOCKING SIGNAL
20DE | PASSENGER DOOR LOCKING SIGNAL
20G | TAILGATE MOTOR OPEN CONTROL
20M | DOOR LOCKING LED
20S | TAILGATE MOTOR OPENING AUTHORISED FEED
21AA | DRIVER ELECTRIC WINDOW RAISE/LOWER CONTROL
21C | ONE-TOUCH ELECTRIC WINDOW NORMAL UP - CONTROL
21E | ONE-TOUCH ELECTRIC WINDOW NORMAL DOWN - CONTROL
21ZA | WINDOW WINDER THERMAL PROTECTION SIGNAL 1
21ZB | WINDOW WINDER THERMAL PROTECTION SIGNAL
22A | PASSENGER'S ELECTRIC WINDOW UP CONTROL
22AA | PASSENGER ELECTRIC WINDOW RAISE/LOWER CONTROL
22B | PASSENGER'S ELECTRIC WINDOW DOWN CONTROL
23A | ELECTRIC WINDOW CONTROL > RIGHT-HAND REAR QUARTER LIGHT CLOSE
23AA | REAR RIGHT-HAND ELECTRIC WINDOW RAISE/LOWER CONTROL
23B | ELECTRIC WINDOW DOWN CONTROL > RIGHT HAND REAR QUARTER LIGHT OPEN
23BA | REAR LEFT-HAND ELECTRIC WINDOW RAISE/LOWER CONTROL
23C | ELECTRIC WINDOW UP CONTROL > LEFT HAND REAR QUARTER LIGHT CLOSE
23D | ELECTRIC WINDOW DOWN CONTROL > LEFT HAND REAR QUARTER LIGHT OPEN
23G | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 1
23H | RIGHT HAND REAR ELECTRIC WINDOW CONTROL 2
23J | LEFT HAND REAR ELECTRIC WINDOW CONTROL 1
23K | LEFT HAND REAR ELECTRIC WINDOW CONTROL 2
23X | REAR LEFT-HAND ANTI-PINCH WINDOW WINDER SERIES SIGNAL
24A | REAR SCREEN WASHER PUMP + CONTROL
26AA | KEYLESS VEHICLE DRIVER'S FRONT DOOR EXTERNAL AERIAL A SIGNAL
26AB | KEYLESS VEHICLE DRIVER'S SIDE FRONT DOOR EXTERNAL AERIAL B SIGNAL
26AC | KEYLESS VEHICLE FRONT PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
26AD | KEYLESS VEHICLE FRONT RIGHT DOOR EXTERNAL AERIAL SIGNAL 2
26AG | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL A SIGNAL
26AH | KEYLESS VEHICLE DRIVER'S SIDE REAR DOOR EXTERNAL AERIAL B SIGNAL
26AK | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL A SIGNAL
26AL | KEYLESS VEHICLE REAR PASSENGER DOOR EXTERNAL AERIAL B SIGNAL
26AM | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL A SIGNAL
26AN | KEYLESS VEHICLE BOOT LID EXTERNAL AERIAL SIGNAL2
26AR | KEYLESS VEHICLE LEVEL 2 LOCKING SIGNAL / BOOT LID SWITCH
26AT | KEYLESS VEHICLE INTERIOR AERIAL 1 SIGNAL 1
26AU | KEYLESS VEHICLE FRONT INTERIOR AERIAL SIGNAL 2
26AV | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 1
26AW | KEYLESS VEHICLE INTERIOR AERIAL 2 SIGNAL 2
26AX | KEYLESS VEHICLE INTERIOR AERIAL 3 SIGNAL 1
26AY | KEYLESS VEHICLE CENTRAL INTERIOR AERIAL SIGNAL 2
26B | CARD PRESENT + SIGNAL
26BD | UCH SYNCHRONISATION / CARD READER SIGNAL
26BG | UCH DATA / CARD READER SIGNAL
26BH | + CARD READER
26BK | - CARD READER
26BM | OIL PRESSURE WARNING LIGHT/ALTERNATOR CHARGING INDICATOR LIGHT CONTROL
26CE | DRIVER'S DOOR SWITCH/LOCKING SIGNAL
26CG | PASSENGER DOOR SWITCH/LOCKING SIGNAL
26CJ | DRIVER'S REAR DOOR SWITCH/LOCKING SIGNAL
26CK | PASSENGER REAR DOOR SWITCH/LOCKING SIGNAL
26H | RADIO FREQUENCY SIGNAL
26HB | RADIO FREQUENCY UNIT SUPPLY
26I | + STEERING COLUMN LOCK
26LA | PASSENGER COMPARTMENT COMMUNICATION SIGNAL/COLUMN LOCK
26LB | COLUMN STATUS SIGNAL 1
26LC | COLUMN STATUS SIGNAL 2
26M | ENGINE RUNNING WARNING LIGHT CONTROL
26N | ENGINE START/STOP + SIGNAL
26P | DOOR HANDLE INFRARED SENSOR +
26Q | PASSENGER SIDE DOOR HANDLE INFRARED SENSOR SIGNAL
26R | RIGHT HAND REAR HANDLE INFRARED SENSOR SIGNAL
26S | DRIVER'S SIDE REAR HANDLE INFRARED SENSOR SIGNAL
26T | DRIVER'S HANDLE INFRARED SENSOR SIGNAL
26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL
27A | HANDBRAKE WARNING LIGHT - CONTROL
28A | OIL PRESSURE WARNING LIGHT - CONTROL
30A | BRAKE FLUID LEVEL WARNING LIGHT - CONTROL
32B | OIL LEVEL SENSOR SIGNAL 1
34A | LEFT HAND REAR LOUDSPEAKER + SIGNAL
34AO | RADIO SATELLITE L3 (LINE 3) SIGNAL
34AP | RADIO SATELLITE SIGNAL L0
34AQ | RADIO SATELLITE SIGNAL L1
34AR | RADIO SATELLITE SIGNAL L2
34AS | RADIO SATELLITE IN0 SIGNAL
34AT | RADIO SATELLITE IN1 SIGNAL
34AU | RADIO SATELLITE IN2 SIGNAL
34B | LEFT HAND REAR LOUDSPEAKER - SIGNAL
34BG | COMPACT DISC AUDIO SIGNAL
34BH | - AUDIO 1 COMPACT DISC
34BL | COMPACT DISC SHIELDING
34C | RIGHT HAND REAR LOUDSPEAKER - SIGNAL
34D | RIGHT HAND REAR LOUDSPEAKER + SIGNAL
34DB | RED RGB SIGNAL
34DC | GREEN RGB VIDEO SIGNAL
34DD | BLUE RGB VIDEO SIGNAL
34E | RIGHT HAND FRONT LOUDSPEAKER + SIGNAL
34EH | SPEAKER + SIGNAL (BASS SECTION)
34EJ | SPEAKER - SIGNAL (BASS SECTION)
34EL | SPEAKER AMPLIFIER CONTROL (BASS SECTION)
34EV | RIGHT-HAND FRONT SPEAKER + SIGNAL (TWEETER)
34EW | RIGHT-HAND FRONT SPEAKER - SIGNAL (TWEETER)
34EX | LEFT-HAND FRONT SPEAKER + SIGNAL (TWEETER)
34EZ | LEFT-HAND FRONT SPEAKER - SIGNAL (TWEETER)
34F | RIGHT HAND FRONT LOUDSPEAKER - SIGNAL
34G | LEFT HAND FRONT LOUDSPEAKER + SIGNAL
34GU | RGB VIDEO SIGNAL EARTH (RED GREEN BLUE)
34GV | VIDEO LIGHTING SIGNAL
34GW | VIDEO DIMMING SIGNAL 1
34GX | VIDEO DIMMING SIGNAL 2
34GZ | REMINDER
34H | LEFT HAND FRONT LOUDSPEAKER - SIGNAL
34HA | VIDEO DISPLAY CONTROL SIGNAL 2
34HB | + TELEPHONE VOICE
34HC | + TELEPHONE VOICE
34HD | - NAVIGATION VOICE
34HG | + NAVIGATION VOICE
34HK | - INFRARED REMOTE CONTROL
34HL | + INFRARED REMOTE CONTROL
34HR | CD CONTROLS CONTROL SIGNAL
34HS | CD TRANSMISSION CONTROL SIGNAL
34HT | CD RECEPTION CONTROL SIGNAL
34HU | MULTIMEDIA WAKE-UP SIGNAL
34HY | MULTIMEDIA STOP/START CONTROL
34JK | RIGHT-HAND AUDIO + SIGNAL
34JL | RIGHT-HAND AUDIO - SIGNAL
34JM | LEFT-HAND AUDIO + SIGNAL
34JP | LEFT-HAND AUDIO - SIGNAL
34KQ | CENTRAL SPEAKER + SIGNAL
34KR | CENTRAL SPEAKER - SIGNAL
34KU | TELEVISION CAN H SIGNAL (TUNER)
34KV | TELEVISION CAN L SIGNAL (TUNER)
34KW | MULTIMEDIA KEYPAD CAN H SIGNAL
34KX | MULTIMEDIA KEYPAD CAN L SIGNAL
34LA | EXTERIOR AMPLIFIER RETURN CONTROL
34LB | + EXTERIOR AMPLIFIER RIGHT-HAND AUDIO
34LC | - EXTERIOR AMPLIFIER RIGHT-HAND AUDIO
34LD | + EXTERIOR AMPLIFIER LEFT-HAND AUDIO
34LE | - EXTERIOR AMPLIFIER LEFT-HAND AUDIO
34LM | EXTERIOR RIGHT-HAND REAR AMPLIFIER AUDIO + SIGNAL
34LP | EXTERIOR RIGHT-HAND REAR AMPLIFIER AUDIO - SIGNAL
34LQ | EXTERIOR LEFT-HAND REAR AMPLIFIER AUDIO + SIGNAL
34LR | EXTERIOR LEFT-HAND REAR AMPLIFIER AUDIO - SIGNAL
34LT | EXTERIOR AMPLIFIER FRONT AUDIO SHIELDING
34LU | EXTERIOR AMPLIFIER REAR AUDIO SHIELDING
34MA | RADIO SOCKET AUXILIARY INPUT SIGNAL
34MB | RADIO SOCKET AUXILIARY INPUT SIGNAL
34MC | HEADPHONE AUXILIARY INPUT EARTH
35A | FRONT PARKING PROXIMITY DETECTOR SENSOR + FEED
35B | FRONT PARKING PROXIMITY DETECTOR SENSOR - FEED
35C | FRONT RIGHT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 3 SIGNAL
35D | FRONT LEFT-HAND INTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 2 SIGNAL
35G | FRONT LEFT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 1 SIGNAL
35H | FRONT RIGHT-HAND EXTERIOR PARKING PARKING PROXIMITY DETECTOR SENSOR 4 SIGNAL
35N | FRONT LOUDSPEAKER SIGNAL
36A | REAR WIPER + CONTROL
36C | REAR SCREEN WIPER PARK POSITION SWITCH - SIGNAL
37AA | PRE-HEATER PLUG 2 CONTROL
37AB | PRE-HEATER PLUG 3 CONTROL
37AC | PRE-HEATER PLUG 4 CONTROL
37Z | PRE-HEATER PLUG 1 CONTROL
38AH | FAN MOTOR SPEED 1 + CONTROL
38AJ | FAN MOTOR SPEED 2 + CONTROL
38AK | FAN MOTOR SPEED 3 + CONTROL
38AL | FAN MOTOR SPEED 4 + CONTROL
38AN | AIR CONDITIONING RECIRCULATION - CONTROL
38AP | AIR CONDITIONING EVAPORATOR SENSOR + SIGNAL
38AY | FAN SPEED SIGNAL
38E | AIR CONDITIONING RECIRCULATION +
38EV | AIR RECIRCULATION + CONTROL
38EW | 0 VOLT EVAPORATOR TEMPERATURE SENSOR CLIMATE CONTROL SIGNAL
38FC | PASSENGER COMPARTMENT FAN CONTROL > RELAY
38GX | SUN SENSOR SIGNAL
38GZ | INTERIOR TEMPERATURE SENSOR SIGNAL
38JA | RECIRCULATION MOTOR CONTROL 1
38JB | RECIRCULATION MOTOR CONTROL 2
38JP | PASSENGER COMPARTMENT RECIRCULATION FAN MOTOR SPEED 1 CONTROL
38JS | CONTROL 1 REAR DISTRIBUTION MOTOR
38JU | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 1
38JV | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 2PASSENGER
38JW | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 3
38K | AIR CONDITIONING CUT-OFF CONTROL > PETROL-DIESEL COMPUTER
38KP | -AIR VENT POSITION SENSOR
38KQ | +AIR VENT POSITION SENSOR
38KS | RIGHT-HAND AIR VENT POSITION SIGNAL
38KY | AIR DISTRIBUTION MOTOR B2 COIL CONTROL
38KZ | AIR DISTRIBUTION MOTOR A2 COIL CONTROL
38LA | AIR DISTRIBUTION MOTOR B1 COIL CONTROL
38LB | AIR DISTRIBUTION MOTOR A1 COIL CONTROL
38LL | PASSENGER COMPARTMENT HEATING RESISTANCE / RELAY 1 CONTROL
38LM | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL / RELAY 2
38LN | PASSENGER COMPARTMENT HEATING RESISTOR CONTROL THOUGH RELAY 3
38LP | AIR CONDITIONING STOP/START CONTROL
38LQ | FAN ASSEMBLY SPEED 0 SIGNAL
38MH | REAR AIR CONDITIONING SOLENOID VALVE CONTROL
38NC | HEATING AND AIR CONDITIONING SYSTEM/ EVAPORATOR SAFETY MODULE ON-OFF COMMAND
38NG | CLIMATE CONTROL PRESENCE DETECTOR SIGNAL
38NH | INSTRUMENT PANEL COOLANT TEMPERATURE SIGNAL
38PR | REAR FAN SPEED SIGNAL
38PS | FAN + CONTROL (REAR AIR CONDITIONING CONTROL PANEL)
38PT | FAN - CONTROL (REAR AIR CONDITIONING CONTROL PANEL)
38QB | REAR MIXER MOTOR B2 COIL CONTROL
38QC | REAR MIXER MOTOR A2 COIL CONTROL
38QD | REAR MIXER MOTOR B1 COIL CONTROL
38QE | REAR MIXER MOTOR A1 COIL CONTROL
38SA | RECIRCULATION MOTOR + SUPPLY
38SQ | LEFT-HAND MIXER MOTOR B2 COIL CONTROL
38SR | LEFT-HAND MIXER MOTOR A2 COIL CONTROL
38SS | LEFT-HAND MIXER MOTOR B1 COIL CONTROL
38ST | LEFT-HAND MIXER MOTOR A1 COIL CONTROL
38U | RHEOSTAT CURSOR
38X | REFRIGERANT GAS PRESSURE SENSOR SIGNAL
38Y | REFRIGERANT GAS PRESSURE SENSOR +
39A | HEADLIGHT WASHER PUMP + CONTROL
39G | HEADLIGHT WASHERS RELAY 1 + CONTROL
3AA | INJECTION LOCKING RELAY COIL - CONTROL
3AAQ | +PARTICLE FILTER DIFFERENTIAL PRESSURE SENSOR
3AAS | UPSTREAM DIESEL OXYGEN SENSOR HEATING-CONTROL
3AAT | UPSTREAM DIESEL OXYGEN SENSOR OUTPUT VOLTAGE
3AAU | UPSTREAM DIESEL OXYGEN SENSOR COMPENSATION RESISTOR SIGNAL
3AAV | -UPSTREAM DIESEL OXYGEN SENSOR
3AAW | DOWNSTREAM DIESEL OXYGEN SENSOR HUNTING CURRENT SIGNAL
3AAX | + SWIRL FLAP MOTOR + CONTROL
3AAY | -SWIRL FLAP MOTOR - CONTROL
3AAZ | WATER PUMP RELAY/FUEL PRESSURE ADJUSTMENT- CONTROL
3ABQ | AIR FLOW TEMPERATURE SIGNAL
3ABS | TURBO UPSTREAM TEMPERATURE SENSOR + SIGNAL
3ABT | - TURBO UPSTREAM TEMPERATURE SENSOR
3ACN | TDC SENSOR/ENGINE SPEED + SIGNAL
3AJB | THROTTLE MOTOR + CONTROL
3AJC | THROTTLE MOTOR - CONTROL
3AKD | BYPASS SOLENOID VALVE - CONTROL (HYDROCARBON REDUCTION SYSTEM)
3B | AIR TEMPERATURE SENSOR + SIGNAL
3BB | CANISTER BLEED SOLENOID VALVE
3BG | ENGINE SPEED SIGNAL > TDC SENSOR
3BL | ENGINE SPEED > TDC SENSOR - SIGNAL
3BS | IGNITION COIL CONTROL
3C | COOLANT TEMPERATURE SENSOR + SIGNAL
3CQ | CAMSHAFT SENSOR SIGNAL
3CR | INJECTOR 1 - CONTROL
3CS | INJECTOR 2 - CONTROL
3CT | INJECTOR 3 - CONTROL
3CU | INJECTOR 4 - CONTROL
3CVA | INJECTOR IGNITION COIL 1 - CONTROL
3CVB | INJECTOR IGNITION COIL 4 - CONTROL
3CWA | INJECTOR IGNITION COIL 2 - CONTROL
3CWB | INJECTOR IGNITION COIL 3 - CONTROL
3DQ | PINKING SENSOR -
3DU | AIRFLOW SENSOR -
3DV | AIRFLOW SENSOR + SIGNAL
3DW | AIRFLOW SENSOR - SIGNAL
3EL | EGR POTENTIOMETER + SIGNAL
3FAB | FUEL TEMPERATURE + SIGNAL
3FB | INJECTION + > PROTECTIVE RELAY
3FB1 | INJECTION + > PROTECTIVE RELAY
3FB2 | INJECTION + > PROTECTIVE RELAY
3FF | PRE-HEATER RELAY - CONTROL
3FJ | INJECTION COMPUTER SENSOR -
3FX | CRUISE CONTROL ON>OFF - CONTROL
3FY | PRE-HEATER RELAY DIAGNOSTIC SIGNAL
3GC | EGR SENSOR +
3GF | UPSTREAM OXYGEN SENSOR HEATER - CONTROL
3GG | DOWNSTREAM OXYGEN SENSOR HEATER - CONTROL
3GH | UPSTREAM OXYGEN SENSOR EARTH
3GJ | DOWNSTREAM OXYGEN SENSOR EARTH
3GK | UPSTREAM OXYGEN SENSOR SIGNAL
3GL | DOWNSTREAM OXYGEN SENSOR SIGNAL
3HI | FUEL PRESSURE CONTROL SOLENOID VALVE - CONTROL
3JK | COOLANT TEMPERATURE -
3JM | EGR SOLENOID VALVE -
3KG | INLET FLAP SOLENOID VALVE - CONTROL
3KW | INJECTOR 1 CONTROL
3KX | INJECTOR 2 CONTROL
3KY | INJECTOR 3 CONTROL
3KZ | INJECTOR 4 CONTROL
3LD | FUEL TEMPERATURE SENSOR -
3LN | TURBOCHARGER PRESSURE SENSOR -
3LP | TURBOCHARGER PRESSURE SENSOR + SIGNAL
3LQ | TURBOCHARGER PRESSURE SENSOR +
3LR | + LOAD POTENTIOMETER 1
3LS | LOAD POTENTIOMETER 1 + SIGNAL
3LT | - LOAD POTENTIOMETER 1
3LU | + LOAD POTENTIOMETER 2
3LV | - LOAD POTENTIOMETER 2
3LW | LOAD POTENTIOMETER 2 + SIGNAL
3LX | RAIL FUEL PRESSURE SENSOR +
3LY | RAIL FUEL PRESSURE SENSOR + SIGNAL
3LZ | RAIL FUEL PRESSURE SENSOR -
3M | CANISTER BLEED SOLENOID VALVE - CONTROL (PETROL VAPOUR ABSORBER)
3MG | TURBO PRESSURE SOLENOID VALVE - CONTROL
3MN | MOTORISED THROTTLE POTENTIOMETER + 5 VOLTS
3MO | MOTORISED THROTTLE POTENTIOMETER SENSOR -
3MP | MOTORISED THROTTLE POTENTIOMETER 1 SIGNAL
3MQ | MOTORISED THROTTLE POTENTIOMETER 2 SIGNAL
3MX | +5V TURBOCHARGER PRESSURE SENSOR
3MY | TURBOCHARGER PRESSURE SENSOR SIGNAL
3MZ | - TURBOCHARGER PRESSURE SENSOR
3N | FUEL PUMP +
3NA | IMPACT SENSOR IGNITION COIL + > FUEL PUMP RELAY
3NAA | +5V TANK PRESSURE SENSOR
3NAB | TANK PRESSURE SENSOR SIGNAL
3NAD | FUEL TEMPERATURE/TANK PRESSURE - SENSOR
3PD | SPEED LIMITER ON/OFF CONTROL
3QK | + CAMSHAFT SENSOR SIGNAL
3RG | PRESSURE RAIL (COMMON RAIL) CONTROL- ADJUSTMENT
3S | PINKING SENSOR 1 + SIGNAL > FRONT
3SV | INLET CAMSHAFT SENSOR SIGNAL
3SX | - INLET CAMSHAFT SENSOR
3SZ | VARIABLE INLET CAMSHAFT CONTROL
3TD | PARTICLE FILTER UPSTREAM TEMPERATURE SENSOR SIGNAL
3TG | PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR SIGNAL
3TL | PARTICLE FILTER DIFFERENTIAL PRESSURE SIGNAL
3TM | -PARTICLE FILTER DIFFERENTIAL PRESSURE SENSOR
3VH | + TURBOCHARGER BEARING COOLANT PUMP
3VP | CONTROL + GAS RECIRCULATION MOTOR
3VQ | CONTROL - GAS RECIRCULATION MOTOR
3WT | WATER IN DIESEL DETECTION SENSOR SIGNAL
3XT | -PARTICLE FILTER UPSTREAM TEMPERATURE SENSOR
3XU | -PARTICLE FILTER DOWNSTREAM TEMPERATURE SENSOR
40A | DRIVER'S REAR VIEW MIRROR RIGHT>LEFT CONTROL
40AA | REAR-VIEW MIRROR EARTH > REAR VIEW MIRROR ANTI-RETURN DIODE
40B | PASSENGER REAR VIEW MIRROR UP/DOWN CONTROL
40C | DRIVER'S REAR VIEW MIRROR UP/DOWN CONTROL
40D | PASSENGER REAR VIEW MIRROR RIGHT>LEFT CONTROL
40E | REAR VIEW MIRROR MOTOR COMMON
40W | REAR-VIEW MIRROR FOLD IN CONTROL
40X | REAR-VIEW MIRROR FOLD OUT CONTROL
41A | FUEL LEVEL SENDER + SIGNAL
41B | FUEL LEVEL -
46BB | NAVIGATION CAN H SIGNAL 1
46BC | NAVIGATION CAN L SIGNAL
46BY | NAVIGATION CAN H SIGNAL 2
46BZ | NAVIGATION CAN L SIGNAL 2
47F | VEHICLE SPEED SIGNAL
47Y | DRIVING ASSISTANCE DISPLAY + CONTROL
49AB | FAN CONTROL 1
49AC | FAN CONTROL 2
49AD | FAN CONTROL 3
49AG | FAN CONTROL- 2
49BA | FAN CONTROL RELAY 1
49BB | FAN CONTROL RELAY 2
4AQ | ELECTRONIC STABILITY PROGRAM ON/OFF SWITCH - CONTROL
4C | LEFT HAND FRONT WHEEL SENSOR SIGNAL
4CV | YAW SENSOR REFERENCE SIGNAL (DIRECTIONAL STABILITY)
4CW | YAW SENSOR SIGNAL (DIRECTIONAL STABILITY)
4CX | LATERAL ACCELERATION SENSOR SIGNAL
4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION
4CZ | YAW SENSOR + (DIRECTIONAL STABILITY) > LATERAL ACCELERATION
4CZA | CLUSTER SENSOR SERIES CONNECTION + SIGNAL
4CZB | CLUSTER SENSOR SERIES CONNECTION - SIGNAL
4CZG | GRADIENT CONTROL (UP/DOWN) ON/OFF CONTROL
4DS | - YAW SENSOR
4E | LEFT HAND FRONT WHEEL SENSOR +
4G | LEFT HAND REAR WHEEL SENSOR SIGNAL
4GJ | BRAKE LIGHTS ON CONTROL RELAY
4H | LEFT HAND REAR WHEEL SENSOR +
4LA | ELECTRONIC STABILITY CONTROL/4X4 COMPUTER LIN SIGNAL
4M | RIGHT HAND FRONT WHEEL SENSOR SIGNAL
4N | RIGHT HAND FRONT WHEEL SENSOR +
4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL
4T | RIGHT HAND REAR WHEEL SENSOR +
52AJ | REAR DOORS CLOSING CONTROL
52K | CERAMIC SUN ROOF OPENING/CLOSING CONTROL 1
52L | SUN ROOF OPENING/CLOSING CONTROL 2
5BY | GEARBOX OIL TEMPERATURE -
5BZ | GEARBOX OIL TEMPERATURE +
5CZ | SHIFT SOLENOID VALVE SWITCH 1 SIGNAL
5DA | GEARBOX INPUT SPEED SENSOR + SIGNAL
5DF | MULTIFUNCTION SWITCH SIGNAL 1
5DH | MULTIFUNCTION SWITCH SIGNAL 3
5DJ | MULTIFUNCTION SWITCH SIGNAL 4
5DL | MODULATING SOLENOID VALVE 3
5DT | IGNITION KEY LOCKING CONTROL
5DU | GEAR LEVER LOCKING - CONTROL
5DZ | 1ST GEAR ENGAGED SIGNAL
5HG | LOCKING ON/OFF SELECTION SOLENOID VALVE CONTROL
5HH | STEPPER MOTOR COIL A CONTROL
5HK | STEPPER MOTOR COIL B CONTROL
5HL | STEPPER MOTOR COIL C CONTROL
5HM | STEPPER MOTOR COIL D CONTROL
5HN | SENSOR EARTH
5HNA | EARTH SENSOR 2
5HP | CVT COMPUTER CLOCK SIGNAL
5HQ | REPROGRAMMABLE MEMORY SELECTION SIGNAL
5HR | INPUT/OUTPUT DATA SIGNAL
5HT | STARTER RELAY CONTROL
5HU | SECONDARY PRESSURE SENSOR SIGNAL (SECONDARY PULLEY)
5HW | PRIMARY PRESSURE SENSOR SIGNAL (PRIMARY PULLEY)
5HX | + SENSOR FEED
5KB | INCREASE SPEED ONE-TOUCH CONTROL SIGNAL
5KC | DECREASE SPEED ONE-TOUCH CONTROL SIGNAL
5KN | GEAR LEVER SWITCH 1 SIGNAL
5KTA | GEARBOX AUTOMATIC MODE (INSTRUMENT PANEL DISPLAY)
5KTB | GEARBOX MANUAL MODE (INSTRUMENT PANEL DISPLAY)
5KY | SHIFT SOLENOID VALVE SWITCH 2 SIGNAL
5LH | MODULATION SOLENOID VALVE SWITCH 1 SIGNAL
5LM | MODULATION SOLENOID VALVE SWITCH 4 SIGNAL
5LW | - COMMON SOLENOID VALVE
5NT | PRIMARY SPEED SENSOR SIGNAL 1
5PR | SECONDARY SPEED SENSOR SIGNAL
5Q | MODULATING SOLENOID VALVE 1
5R | MODULATING SOLENOID VALVE 2
5T | GEARBOX OUTPUT SPEED SENSOR +
5TA | GEARBOX OUTPUT SPEED SENSOR -
60AK | DRIVER'S LAP STRAP PRETENSIONER + CONTROL
60AL | DRIVER'S LAP STRAP PRETENSIONER - CONTROL
60AM | LEVEL 1 DRIVER'S FRONT AIR BAG + CONTROL
60AN | LEVEL 1 DRIVER'S FRONT AIR BAG - CONTROL
60AR | DRIVER'S SIDE THORAX AIR BAG + CONTROL
60AS | - DRIVER'S SIDE THORAX AIR BAG CONTROL
60B | PASSENGER'S PRETENSIONER + SIGNAL
60BB | PASSENGER'S SIDE THORAX AIR BAG + CONTROL
60BC | PASSENGER'S SIDE THORAX AIR BAG - CONTROL
60BY | DRIVER'S HEAD CURTAIN AIR BAG + CONTROL
60BZ | DRIVER'S HEAD CURTAIN AIR BAG - CONTROL
60C | PASSENGER'S PRETENSIONER _ SIGNAL
60CA | PASSENGER'S HEAD CURTAIN AIR BAG + CONTROL
60CB | PASSENGER'S HEAD CURTAIN AIR BAG - CONTROL
60D | DRIVER'S PRETENSIONER + SIGNAL
60DS | PASSENGER AIR BAG INHIBITOR KEY SIGNAL
60DT | - PASSENGER AIR BAG INHIBITOR KEY
60E | DRIVER'S PRETENSIONER - SIGNAL
60EE | FRONT LEFT-HAND SEAT BELT SENSOR SIGNAL
60EH | FRONT RIGHT-HAND SEAT BELT SWITCH SIGNAL
60ES | FRONT RIGHT-HAND PRESENCE / POSITION EARTH
60H | PASSENGER EUROBAG + SIGNAL
60JF | FRONT FRONTAL SATELLITE + SIGNAL
60JG | FRONT FRONTAL SATELLITE - SIGNAL
60K | PASSENGER'S FRONT AIR BAG LEVEL 1 - CONTROL
60KX | LEFT-HAND SIDE SATELLITE (AIRBAG) + SIGNAL
60KY | LEFT-HAND SIDE SATELLITE (AIRBAG) - SIGNAL
60KZ | RIGHT-HAND SIDE SATELLITE (AIRBAG) + SIGNAL
60LA | RIGHT-HAND SIDE SATELLITE (AIRBAG) - SIGNAL
60PC | PASSENGER AIRBAG OFF WARNING LIGHT CONTROL
60PF | DRIVER'S AIR BAG WARNING LIGHT CONTROL
64C | LEFT HAND TURN SIGNAL LIGHTS CONTROL
64D | RIGHT HAND TURN SIGNAL LIGHTS CONTROL
64Q | FLASHER UNIT TIMER - CONTROL
65A | BRAKE LIGHTS + CONTROL
65G | BRAKE LIGHT CONTROL > RELAY
65Q | STOP SWITCH SIGNAL 2
67A | HORN + CONTROL
67E | + AUDIBLE WARNING RELAYED PROTECTED SUPPLY
67G | ELECTRIC CONTROL UNIT > AUDIBLE WARNING ACTIVATION SIGNAL
70BA | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY
70BB | RIGHT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL
70BC | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL
70BD | RIGHT-HAND FRONT WHEEL AERIAL RECEIVER EARTH
70BE | LEFT-HAND FRONT WHEEL AERIAL RECEIVER + SUPPLY
70BG | LEFT-HAND FRONT WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL
70BK | LEFT-HAND FRONT WHEEL AERIAL RECEIVER SIGNAL
70BL | LEFT-HAND FRONT WHEEL AERIAL RECEIVER EARTH
70BM | RIGHT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY
70BP | RIGHT-HAND REAR RADIO FREQUENCY AMPLITUDE SIGNAL
70BQ | RIGHT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL
70BR | RIGHT-HAND REAR WHEEL AERIAL RECEIVER EARTH
70BS | LEFT-HAND REAR WHEEL AERIAL RECEIVER + SUPPLY
70BT | LEFT-HAND REAR WHEEL RADIO FREQUENCY AMPLITUDE SIGNAL
70BU | LEFT-HAND REAR WHEEL AERIAL RECEIVER SIGNAL
70BV | LEFT-HAND REAR WHEEL AERIAL RECEIVER EARTH
70M | TYRE PRESSURE MONITOR TYRE PRESSURE AUTOMATIC TEST SIGNAL
78H | DAY>NIGHT RELAY CONTROL
79A | HEATED SEAT + CONTROL
79FA | HEATED SEAT WARNING LIGHT CONTROL, LOW POSITION
79FB | HEATED SEAT WARNING LIGHT CONTROL, HIGH POSITION
80A | BONNET SWITCH - SIGNAL
80FG | CENTRAL ELECTRICAL UNIT SIGNAL CODE / UCH COMPUTER CONTROL
85AA | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION + SIGNAL
85AB | INSTRUMENT PANEL/RIDE HEIGHT SENSOR (COMPASS) SERIES CONNECTION EARTH
85D | 4X4 TORQUE CONTROL
85G | 4X4 CLUTCH RELAY CONTROL
85Q | 4X4 MODE SIGNAL
85R | 4X2 MODE SIGNAL
85T | 4X4 SOLENOID VALVE + CONTROL
85U | 4X4 SOLENOID VALVE - CONTROL
85V | 4X4 AUTOMATIC MODE SIGNAL
86D | DECLUTCH + SIGNAL
86G | CRUISE CONTROL PROGRAMMING CONTROL
86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL
86V | CLUTCH POSITION SENSOR SIGNAL
87A | LEFT HAND REAR 1st POSITION SWITCH - SIGNAL
87B | RIGHT HAND REAR 1st POSITION SWITCH - SIGNAL
87G | PASSENGER'S 1st POSITION SWITCH - SIGNAL
87H | DRIVER'S 1st POSITION SWITCH - SIGNAL
87T | BOOT LID POSITION SWITCH 1 SIGNAL
8E | + FRONT LEFT-HAND FOG LIGHTS > RESISTANCE
8F | + FRONT RIGHT-HAND FOG LIGHTS > RESISTANCE
91M | DRIVER'S SEAT BACK UPRIGHTING MOTOR CONTROL
91N | DRIVER'S SEAT BACK LOWERING MOTOR CONTROL
91P | MOTOR CONTROL FOR MOVING DRIVER'S SEAT RUNNER FORWARDS
91Q | MOTOR FOR MOVING DRIVER'S SEAT RUNNER BACKWARDS
91V | SEAT RAISING MOTOR CONTROL
91W | DRIVER'S SEAT LOWERING CONTROL
96L | DRIVER'S SEATBELT REMINDER LIGHT CONTROL
96M | PASSENGER SEAT BELT REMINDER LIGHT CONTROL FEED
9P | PROTECTED REAR FOG LIGHTS + CONTROL
A1 | + AFTER IGNITION ELECTRIC WINDOW FUSE > RELAY
A4 | PASSENGER COMPARTMENT AFTER IGNITION CONTROL RELAY
A5 | ENGINE AFTER IGNITION CONTROL RELAY
AP11 | PROTECTED + AFTER IGNITION REVERSING LIGHTS FUSE
AP15 | PROTECTED + AFTER IGNITION ENGINE FUNCTIONS FUSE
AP17 | PROTECTED + AFTER IGNITION, INJECTION SIMULATOR FUSE
AP1C | PROTECTED + AFTER IGNITION FEED/4X4 COMPUTER
AP25 | PROTECTED + AFTER IGNITION AIR BAG FUSE
AP28 | PROTECTED + AFTER IGNITION FUSE COOLING FAN ASSEMBLY
AP4 | PROTECTED + AFTER IGNITION AUTOMATIC TRANSMISSION FUSE
AP43 | PROTECED + AFTER IGNITION FUSE
AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION
AP45 | + AFTER IGNITION FEED PROTECTED BY FUSE FOR PASSENGER COMPARTMENT FUNCTIONS
AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE
AP7 | PROTECTED + AFTER IGNITION WINDSCREEN WIPER FUSE
APCB | + AFTER IGNITION PROTECTED / COLUMN LOCK FUSE CONTACT CLOSED AT REST
B | + BATTERY FEED
BP1 | PROTECTED + BATTERY FEED > AIR CONDITIONING
BP10 | PROTECTED + BATTERY FEED > DIAGNOSTIC SOCKET
BP12 | PROTECTED + BATTERY FEED > PASSENGER COMPARTMENT 2
BP14 | PROTECTED + BATTERY FEED > ABS
BP1B | + BATTERY PROTECTED > HEATED SEATS
BP1C | + BATTERY PROTECTED > PROTECTION AND SWITCHING UNIT
BP1H | PROTECTED + BATTERY FEED/MULTIMEDIA
BP1Q | PROTECTED + BATTERY FEED/PASSENGER COMPARTMENT STARTING AND AFTER IGNITION
BP1R | PROTECTED + BATTERY FEED/ENGINE AFTER IGNITION
BP1S | PROTECTED + BATTERY FEED / ENGINE INTER-CONNECTION UNIT SHUNT
BP20 | PROTECTED + BATTERY FEED HEADLIGHT WASHERS
BP26 | CARPHONE PROTECTED + BATTERY FEED
BP35 | PROTECTED + BATTERY FEED PRE-HEATER UNIT FUSE
BP42 | PROTECTED + BATTERY FEED > AUTOMATIC TRANSMISSION COMPUTER
BP48 | PROTECTED + BATTERY FEED > ELECTRIC WINDOW
BP6 | PROTECTED + BATTERY FEED > INTERIOR LIGHT
BP69 | PROTECTED BATTERY FEED > INSTRUMENT PANEL > ECU +
BP7 | PROTECTED + BATTERY FEED > FAN FUSE 1
BP71 | PROTECTED + BATTERY FEED > FAN FUSE 2
BP73 | PROTECTED + BATTERY FEED FAN FUSE
BP74 | PROTECTED + BATTERY FEED PASSENGER COMPARTMENT FAN FUSE
BP76 | BATTERY PROTECTED + FEED > LIGHTING CONTROL
BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR
BP81 | PROTECTED + BATTERY FEED > ELECTRIC POWER-ASSISTED STEERING
BP89 | AUTOMATIC PARKING BRAKE FUSE PROTECTED + BATTERY FEED
BP9 | PROTECTED + BATTERY FEED ADDITIONAL HEATER FUSE
BP91 | PROTECTED + BATTERY FEED ADDITIONAL HEATER FUSE
BPA4 | + BATTERY HORN PROTECTED FEED
BPA7 | BRAKE LIGHTS + BATTERY PROTECTED
BPDA | PROTECTED + BATTERY FEED > ALTERNATOR STARTING
BPDB | ALTERNATOR PROTECTED + BATTERY FEED
BPT | PROTECTED + BATTERY FEED TIMER
CANH | DIAGNOSTIC CAN H SIGNAL
CANL | DIAGNOSTIC CAN L SIGNAL
CPD | PROTECTED RIGHT HAND DIPPED BEAM HEADLIGHT +
CPG | PROTECTED LEFT HAND DIPPED BEAM HEADLIGHT +
H47 | VEHICLE SPEED > SECONDARY SPEED SIGNAL
H66P | REVERSING LIGHTS + CONTROL
HK | DIAGNOSTIC SIGNAL K
LP | PROTECTED + SIDE LIGHT FEED
MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH
MAL | ELECTRIC POWER ASSISTED STEERING EARTH STRAP
MAW | REAR RIGHT-HAND WHEEL ARCH RADIO ELECTRICAL EARTH
MK | LEFT-HAND A-PILLAR ELECTRICAL EARTH
MT | RADIO ELECTRICAL EARTH
MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT
MZR | FRONT SIDE MEMBER ELECTRIC EARTH ARRANGEMENT
MZS | LEFT-HAND REAR ELECTRIC EARTH ARRANGEMENT
MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT
MZU | ELECTRIC EARTH ARRANGEMENT, REAR LEFT AND TAILGATE
NAU | LEFT HAND B-PILLAR ELECTRONIC EARTH
NAV | RIGHT HAND B-PILLAR ELECTRONIC EARTH
NUH | FRONT RIGHT-HAND SIDE MEMBER ELECTRONIC EARTH
NV | FRONT LEFT-HAND SIDE MEMBER ELECTRONIC EARTH 3
RPD | RIGHT HAND PROTECTED MAIN BEAM HEADLIGHT +
RPG | LEFT HAND PROTECTED MAIN BEAM HEADLIGHT +
SP16 | PROTECTED + ACCESSORIES FEED / ACCESSORIES FEED FUSE SUPPLY
SP2 | PROTECTED + ACCESSORIES > RADIO
SP4A | ACCESSORIES SOCKET 2 PROTECTED + ACCESSORIES FEED
SP4D | + PROTECTED >ACCESSORIES FEED ACCESSORIES SOCKET 1
SP4G | CIGARETTE LIGHTER PROTECTED + ACCESSORIES FEED
TB26 | TELEPHONE VOICE SHIELDED CABLE
TB27 | NAVIGATION VOICE SHIELDED CABLE
TB29 | CD CONTROLS SHIELDED CABLE
TB30 | VIDEO CONTROL SHIELDED CABLE
TB32 | SHIELDED CABLE
TB38 | SPEAKER SHIELDED CABLE (BASS SECTION)
TB45 | RADIO SOCKET AUXILIARY SOCKET INPUT SHIELDED CABLE
TB46 | TELEVISION IMAGE SHIELDED CABLE