| FRONT WIRING
H45/BVM6/M9R

#### 1094
ANTI-LOCK BRAKING SYSTEM/ELECTRONIC STABILITY PROGRAM COMPUTER
DG/TR4X4/ASRES2/NINAV4/RAD04,RAD05,RAD07

1 | 3.0 | BP8 | PROTECTED + BATTERY FEED > ANTI-LOCK BRAKING SYSTEM MOTOR | ?????
2 | 3.0 | BP14 | PROTECTED + BATTERY FEED > ABS | ?????
3 | 3.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH | ?????
4 | 3.0 | MAH | ANTI-LOCK BRAKING SYSTEM ELECTRICAL EARTH | ?????
5 | 0.5 | 4AQ | ELECTRONIC STABILITY PROGRAM ON/OFF SWITCH - CONTROL | F005E
6 | 0.5 | 65Q | STOP SWITCH SIGNAL 2 | F005E
8 | 0.5 | 65A | BRAKE LIGHTS + CONTROL | F005E
9 | 0.5 | CANL | DIAGNOSTIC CAN L SIGNAL | F005E
11 | 0.5 | 4T | RIGHT HAND REAR WHEEL SENSOR + | F005E
12 | 0.5 | 4M | RIGHT HAND FRONT WHEEL SENSOR SIGNAL | F005E
13 | 0.5 | 4CZ | YAW SENSOR + (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | F005E
14 | 0.5 | 4CZA | CLUSTER SENSOR SERIES CONNECTION + SIGNAL | F005E
15 | 0.5 | 4S | RIGHT HAND REAR WHEEL SENSOR SIGNAL | F005E
16 | 0.5 | AP5 | PROTECTED + AFTER IGNITION ANTI-LOCK BRAKING SYSTEM FUSE | F005E
17 | 0.5 | H66P | REVERSING LIGHTS + CONTROL | F005E
18 | 0.5 | 4CZG | GRADIENT CONTROL (UP/DOWN) ON/OFF CONTROL | F005E
19 | 0.5 | 4GJ | BRAKE LIGHTS ON CONTROL RELAY | F005E
20 | 0.5 | 4LA | ELECTRONIC STABILITY CONTROL/4X4 COMPUTER LIN SIGNAL | F005E
21 | 0.5 | 4N | RIGHT HAND FRONT WHEEL SENSOR + | F005E
22 | 0.5 | CANH | DIAGNOSTIC CAN H SIGNAL | F005E
23 | 0.5 | 4E | LEFT HAND FRONT WHEEL SENSOR + | F005E
25 | 0.5 | 26Z | AUTOMATIC TRANSMISSION NEUTRAL + SIGNAL | F005E
26 | 0.5 | 4H | LEFT HAND REAR WHEEL SENSOR + | F005E
27 | 0.5 | 4C | LEFT HAND FRONT WHEEL SENSOR SIGNAL | F005E
28 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | F005E
29 | 0.5 | 4CZB | CLUSTER SENSOR SERIES CONNECTION - SIGNAL | F005E
30 | 0.5 | 4G | LEFT HAND REAR WHEEL SENSOR SIGNAL | F005E
31 | 0.5 | 5DZ | 1ST GEAR ENGAGED SIGNAL | F005E