| FRONT WIRING
H45/BVM6/M9R

#### 1069
ADDITIONAL HEATING RELAY 3
DG/TR4X4/SSESP/NINAV4/RAD04,RAD05,RAD07

1 | 3.0 | BP91 | PROTECTED + BATTERY FEED ADDITIONAL HEATER FUSE | ?????
2 | 0.5 | 38JW | PASSENGER COMPARTMENT HEATING RESISTANCE CONTROL RELAY 3 | ?????
3 | 0.5 | AP44 | POWER ASSISTED STEERING ECU + AFTER IGNITION FEED FUSE PROTECTION | ?????
4 | 3.0 | 38LN | PASSENGER COMPARTMENT HEATING RESISTOR CONTROL THOUGH RELAY 3 | ?????