| CONNECTION
ANY TYPE

#### R462
PEDALS/DASHBOARD 2
H45/BVVR/2TR DG/TR4X2/ASRES2/NINAV4/RAD04,RAD05,RAD07

1 | 0.3 | 3PD | SPEED LIMITER ON/OFF CONTROL | ?????
2 | 0.5 | MZT | RIGHT-HAND REAR ELECTRIC EARTH ARRANGEMENT | ?????
3 | 0.5 | 4CZB | CLUSTER SENSOR SERIES CONNECTION - SIGNAL | ?????
4 | 0.5 | 4CZ | YAW SENSOR + (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | ?????
5 | 0.5 | 4AQ | ELECTRONIC STABILITY PROGRAM ON/OFF SWITCH - CONTROL | ?????
9 | 0.5 | 32B | OIL LEVEL SENSOR SIGNAL 1 | ?????
10 | 0.5 | 86M | CRUISE CONTROL PROGRAMMING RETURN SIGNAL | ?????
11 | 0.3 | 3FX | CRUISE CONTROL ON>OFF - CONTROL | ?????
12 | 0.5 | 86G | CRUISE CONTROL PROGRAMMING CONTROL | ?????
13 | 0.5 | 4CY | YAW SENSOR - (DIRECTIONAL STABILITY) > LATERAL ACCELERATION | ?????
14 | 0.5 | 4CZA | CLUSTER SENSOR SERIES CONNECTION + SIGNAL | ?????
19 | 0.5 | 115A | OIL TEMPERATURE SENSOR - SIGNAL | ?????
20 | 0.5 | HK | DIAGNOSTIC SIGNAL K | ?????