| FRONT PASSENGER DOOR WIRING
H45/DG

#### 1375
PASSENGER FRONT DOOR HANDS-FREE CARD DETECTION AERIAL
RET01,RET02,RET03/LVILVI/NINAV1/RAD01,RAD02,RAD04,RAD05

1 | 0.3 | MZQ | DASHBOARD ELECTRIC EARTH ARRANGEMENT | F005E
2 | 0.3 | 26CG | PASSENGER DOOR SWITCH/LOCKING SIGNAL | F005E
3 | 0.3 | 26AD | KEYLESS VEHICLE FRONT RIGHT DOOR EXTERNAL AERIAL SIGNAL 2 | F005E
4 | 0.3 | 26AC | KEYLESS VEHICLE FRONT PASSENGER DOOR EXTERNAL AERIAL A SIGNAL | F005E